CHANGE REQUEST	

Request identity number:	
C00222	

Applies to:	
S01886	

Type of request:	
Technically new	

Request status level:	
For evaluation	

Proposal:	
Introduce a alternative form (2) of fluorescent lamp symbol S00484

Reason:	General symbol S00965 for lamp is combination of cross bar and circle. The cross bar is used as part of lamp symbols for installation diagrams almost every case except “Fluorescent lamp” symbol family S00484-S00486. These symbols without cross bar are sometimes difficult to recognized to be symbols for light producing objects. Some CAD software already uses same graphics as it is FI NC proposal.

FI NC propose to standardize alternative form (2) of fluorescent lamp symbol S00484.  	

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	

SYMBOL	

Symbol identity number:	
S01886	
Status:	
Proposed	

Drawing:		

Earlier published in:	
.	
Not applicable 	

Name:	
EN	
Luminaire, general symbol; Fluorescent lamp, general symbol	
	
FR	

Keywords:	
EN	
installations in buildings, lamps, lightning outlets and fittings	
	
FR	

Applies:		S00484, S00481	

Application notes:			
Application class:		Installation diagrams	
Function class:		E Providing radiant or thermal energy	
Shape class		Lines