CHANGE REQUEST	

Request identity number:	
C00251  part 2	

Type of request:	
Editorial change	

Request status level:	
For evaluation	

Proposal:	
Modify title and description of graphical symbol S00471 

Reason:	This change request is part of MT 60617 recommendation to harmonize graphical symbol family "switches for installation diagrams" to make all titles, graphical presentations, descriptions, application notes to be consistent and help users of symbols to choose right symbols particular purpose. 

During the preparation of this proposal MT 60617 was consulted.

FI NC propose to modify S00471 as highlighted below	

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	

SYMBOL	

Symbol identity number:	
S00471	
Status:	
Standard	

Drawing:		

Earlier published in:	
.	
IEC 60617-11 (ed.2.0) 11-14-06 	

Name:

Alternative names:	
EN

EN	
Two-way single pole switch
Interrupteur unipolaire va-et-vient

Change over single pole switch
Changez du plus commutateur de poteau simple	

Keywords:	
EN	
installations in buildings, switches	

Applies:

Applied in:

Application note:		 
S00466

S01868, S01869

A00266, A00366	
Application class:		Installation diagrams	
Function class:		Q Controlled switching or varying, 
S Converting a manual operation into a signal	
Shape class:

		Circles, Lines

APPLICATION NOTE	

Note identity number:	
A00366	
Status:	
Proposed 	
Note type:	General			

Note (EN):

Graphical symbol S00471, for use in installation diagrams, represents a device (switch) which has one actuator operating one swith-over contact. The function of such device is illustrated in attached File

See Circuit diagram presentation of symbol S004471: A00366 Illustration

Circuit diagram presentation on symbol S00471

Applies to: S00471