CHANGE REQUEST	

Request identity number:	
C00251 part 4	

Type of request:	
Editorial change	

Request status level:	
For evaluation	

Proposal:	
Modify title and description of graphical symbol S00474 

Reason:	This change request is part of MT 60617 recommendation to harmonize graphical symbol family "switches for installation diagrams" to make all titles, graphical presentations, descriptions, application notes to be consistent and help users of symbols to choose right symbols particular purpose. 

During the preparation of this proposal MT 60617 was consulted.

FI NC propose to modify S00474 as highlighted below	

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	

SYMBOL	

Symbol identity number:	
S00474	
Status:	
Standard	

Drawing:		

Earlier published in:	
.	
IEC 60617-11 (ed.2.0) 11-14-09 	

Name:	
EN	
Pull-cord single pole switch

Keywords:	
EN	
installations in buildings, switches	

Applies:

Application note:		 
S00093, S00466

A00266, A00367	
Application class:		Installation diagrams	
Function class:		Q Controlled switching or varying, 
S Converting a manual operation into a signal	
Shape class:

		Arrows, Circles, Lines

APPLICATION NOTE	

Note identity number:	
A00367	
Status:	
Proposed	
Note type:	General			

Note (EN):

Graphical symbol S00474, for use in installation diagrams, represents a device (switch) which has a single actuator. The function of such device is illustrated in attached File

See Circuit diagram presentation of symbol S004474: A00367 Illustration

Circuit diagram presentation on symbol S00474

Applies to: S00474