CHANGE REQUEST	

Request identity number:	
C00267	

Type of request:	
Technically new	

Request status level:	
For evaluation	

Proposal:	
Proposal to standardize graphical symbol Connection, built-in mounted 

Reason:	This CR use graphical presentation of symbol S01448 with new meaning: Connection, flush mounted or connector built-in behind a surface e.g. a wall

During the preparation of this proposal MT 60617 was consulted

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	

SYMBOL	

Symbol identity number:	
S01916	
Status:	
Proposed	

Drawing:		

Earlier published in:	
.	
Not applicable 	

Name:	
EN	
Connection, behind surface	

Alternative names:	
EN	
Flush mounted connector	

Keywords:	
EN	
connection, line, cable, wire	

Applies:		 
S00001	
Application class:		Installation diagrams	
Function class:		X Connecting 	
Shape class		Lines, depicting shapes