CHANGE REQUEST	

Request identity number:	
C00246	

Type of request:	
Technical change	

Request status level:	
For evaluation	

Proposal:	
(Modify symbol, title and description of graphical symbol S00467)
Add a new symbol based on symbol S00467 

Reason:	This change request is part of MT 60617 recommendation to harmonize graphical symbol family "switches for installation diagrams" to make all titles, graphical presentations, descriptions, application notes to be consistent and help users of symbols to choose right symbols particular purpose. 

During the preparation of this proposal MT 60617 was consulted.

FI NC propose to replace graphical symbol S00467 by following new graphical symbol	

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	

SYMBOL	

Symbol identity number:	
S01907	
Status:	
Standard	

Drawing:		

Earlier published in:	
.	
Not applicable	

Name:	
EN	
Single pole switch with signal lamp
Interrupteur de poteau simple à lampe de signal	

Keywords:	
EN	
indicator lamps, installations in buildings, switches	

Applies:

Application notes:		 
S00466, S00965

A00266, A00364	
Application class:		Installation diagrams	
Function class:		Q Controlled switching or varying, 
S Converting a manual operation into a signal	
Shape class:

Replacing:

		Circles, Lines

S00467

APPLICATION NOTE	

Note identity number:	
A00364	
Status:	
Proposed     	
Note type:	General			

Note (EN):

Graphical symbol S01907, for use in installation diagrams, represents a device (switch) which has one actuator and one lamp. The function of such device is illustrated in attached File

See Circuit diagram presentation of symbol S00467: A00364 Illustration

Circuit diagram presentation on symbol S00467