CHANGE REQUEST	

Request identity number:	
C00245	

Type of request:	
Technically new	

Request status level:	
For evaluation	

Proposal:	
Introduce a new symbol for concept: Triple two-way single pole switch

Reason:	This change request is part of MT 60617 recommendation to harmonize graphical symbol family "switches for installation diagrams" to make all titles, graphical presentations, descriptions, application notes to be consistent and help users of symbols to choose right symbols particular purpose. 

During the preparation of this proposal MT 60617 was consulted.

FI NC propose to standardize a graphical symbol for triple two-way single pole switch	

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	

SYMBOL	

Symbol identity number:	
S01901	
Status:	
Standard	

Drawing:		

Earlier published in:	
.	
Not applicable	

Name:

Alternative names:	
EN

EN	
Triple two-way single pole switch
Triple interrupteur unipolaire va-et-vient

Triple change over single pole switch
Triple Changez du plus commutateur de poteau simple	

Keywords:	
EN	
installations in buildings, switches	

Applies:

Application note:		 
S00471

A00266, A00363	
Application class:		Installation diagrams	
Function class:		Q Controlled switching or varying, 
S Converting a manual operation into a signal	
Shape class:

		Circles, Lines

APPLICATION NOTE	

Note identity number:	
A00363	
Status:	
Proposed 	
Note type:	General			

Note (EN):

Graphical symbol S01901, for use in installation diagrams, represents a device (switch) which has triple actuators. The function of such device is illustrated in attached File

See Circuit diagram presentation of symbol S01901: A00363 Illustration

Circuit diagram presentation on symbol S01901

Applies to: S01901