CHANGE REQUEST	

Request identity number:	
C00242	

Type of request:	
Technical change	

Request status level:	
For evaluation	

Proposal:	
Modify graphical presentation, title and description of graphical symbol S01862. 

Reason:	This change request is part of MT 60617 recommendation to harmonize graphical symbol family "switches for installation diagrams" to make all titles, graphical presentations, descriptions, application notes to be consistent and help users of symbols to choose right symbols particular purpose. 

During the preparation of this proposal MT 60617 was consulted.

FI NC propose to replace graphical symbol S01862 by following new graphical symbol	

Requested by:

Note: 	
Arto Sirviö
arto.sirvio@sesko.fi
FI

Show the replaced symbol S01862 in this Change request	

SYMBOL	

Symbol identity number:	
S01906	
Status:	
Proposed	

Drawing:		

Earlier published in:	
.	
Not applicable 	

Name:

Alternative name	
EN

EN	
Triple single pole switch
Triple Commutateur de poteau simple 

Triple On-Off switch
Commutateur marche-arrêt triple	

Keywords:	
EN	
installations in buildings, switches	

Applies:

Application note:		 
S00466

A00266, A00361	
Application class:		Installation diagrams	
Function class:		Q Controlled switching or varying, 
S Converting a manual operation into a signal	
Shape class:

Replacing:

		Circles, Lines

S01862

APPLICATION NOTE	

Note identity number:	
A00361	
Status:	
Proposed 	
Note type:	General			

Note (EN):

Graphical symbol S01862, for use in installation diagrams, represents a device (switch) which has triple actuators. The function of such device is illustrated in attached File

See Circuit diagram presentation of symbol S01862: A00361 Illustration.
.

Circuit diagram presentation on symbol S01906

Applies to: S01906