CHANGE REQUEST	

Request identity number:	
C00250     (part 2)	

Type of request:	
Editorial change	

Request status level:	
For evaluation	

Proposal:	
Modify title and description of graphical symbol S00467 

Reason:	This change request is part of MT 60617 recommendation to harmonize graphical symbol family "switches for installation diagrams" to make all titles, graphical presentations, descriptions, application notes to be consistent and help users of symbols to choose right symbols particular purpose. 

During the preparation of this proposal MT 60617 was consulted.

FI NC propose to modify S00467 as highlighted below	

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	

SYMBOL	

Symbol identity number:	
S00467	
Status:	
Standard	

Drawing:		

Earlier published in:	
.	
IEC 60617-11 (ed.2.0) 11-14-02 	

Name:

Alt name	
EN

EN	
Switch with signal lamp, general symbol installation diagram
Interrupteur à lampe de signal, symbole general de schémas d'installations

Switch with pilot light, genaera symbol installation digram
Interrupteur à lampe témoin, symbole general de schémas d'installations	

Keywords:	
EN	
indicator lamps, installations in buildings, switches	

Applies:		 
S00466, S00965	
Application class:		Installation diagrams	
Function class:		Q Controlled switching or varying, 
S Converting a manual operation into a signal	
Shape class:

Remarks:		Circles, Lines

In this graphical symbol number of poles is not presented