CHANGE REQUEST	

Request identity number:	
C00236	

Applies to:	
A00357	

Type of request:	
Technically new	

Request status level:	
For evaluation	

Proposal:	
Introduce a new Application note of type “Rule”
To be applied symbol ID: S01870 (Detector, General symbol)	

Reason:	
To instruct about application of qualifying symbols to be used for indicating the type of detector 	

Requested by:	
Arto Sirviö
arto.sirvio@sesko.fi
FI	
Application Note	
Note identity number:	A00357			

Note ID:		A00357	
Note Type:		Rule	
Note:	EN	The asterisk shall be replaced by one or more following qualifying symbols to indicating the type of the detector:
- S01851 Heat (occurrence of), general symbol see S01882
- S01852 Smoke (occurrence of), general symbol see S01874
- S01853 Flame (occurrence of), general symbol see S01881
- S01854 Motion (occurrence of), general symbol see S01871	
	FR	L'astérisque sera remplacé par un ou plusieurs des symboles de qualification suivants à indiquer le type du détecteur : 
- La chaleur S01851 (occurrence de), symbole général voient S01882 
- La fumée S01852 (occurrence de), symbole général voient S01874 
- La flamme S01853 (occurrence de), symbole général voient S01881 
- Le mouvement S01854 (occurrence de), symbole général voient S01871 	
Applies to:		S01870